Document: Extra Items

|  |  |
| --- | --- |
| Field | Value |
| extra\_items | {'serial\_no': 'E-01', 'reference': '', 'description': ' Minimum lumen output 2500 Im Post top Luminarie', 'quantity': 2.0, 'unit': 'Each', 'rate': 5075.0, 'amount': 10150.0, 'remark': ''}; {'serial\_no': 'E-02', 'reference': '', 'description': '6 A 3/5 pin shuttered socket', 'quantity': 4.0, 'unit': 'Each', 'rate': 107.0, 'amount': 428.0, 'remark': ''}; {'serial\_no': 'E-03', 'reference': '', 'description': '6/16 A shuttered socket', 'quantity': 5.0, 'unit': 'Each', 'rate': 176.0, 'amount': 880.0, 'remark': ''}; {'serial\_no': 'E-04', 'reference': '', 'description': "Providing & Fixing of modular type lockable feature socket duly made out of unbreakable and fire retardant vergin poly carbonate with brass terminals and captive screws & silver alloy contact tip with IP-20 rating, including all as per pre approved by Engineer in charge, making connections, testing etc. as required. For additional technical parameters of product / work refer Annexure 'A' attached with this BSR", 'quantity': 5.0, 'unit': 'Each', 'rate': 345.0, 'amount': 1725.0, 'remark': ''}; {'serial\_no': 'E-05', 'reference': '', 'description': '6 A 3/5 pin shuttered socket', 'quantity': 4.0, 'unit': 'Each', 'rate': 107.0, 'amount': 428.0, 'remark': ''}; {'serial\_no': 'E-06', 'reference': '', 'description': '6/16 A shuttered socket', 'quantity': 5.0, 'unit': 'Each', 'rate': 176.0, 'amount': 880.0, 'remark': ''} |
| grand\_total | 14491.0 |
| tender\_premium\_percent | 0.04 |
| tender\_premium | 579.64 |
| total\_executed | 15070.64 |